{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"List1","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[[1,1,1,2],[34,1,34,2],[36,1,36,2],[26,1,26,2],[16,1,16,2],[14,1,14,2],[10,1,10,2]]}
[]
[null,"Omytí zdiva tlakovou vodou",null,{"$f":"SUM(D3:D10)","v":523.39189999999996},"m2"]
[null,"jižní strana vnější","(22,0+22,0)*1,2",{"$f":"VYPOCET(C3)","v":52.8},"m2"]
[null,"západní strana vnější","66,36*1,1",{"$f":"VYPOCET(C4)","v":72.996000000000009},"m2"]
[null,"východní a severní strana vnitřní","(11,358+27,199+47,232)*1,1",{"$f":"VYPOCET(C5)","v":94.367900000000006},"m2"]
[null,"západní strana vnitřní","54,64*1,2",{"$f":"VYPOCET(C6)","v":65.567999999999998},"m2"]
[null,"jižní strana vnitřní","(4,8+6,848+0,8+0,8+0,8+1)*1,2",{"$f":"VYPOCET(C7)","v":18.057600000000001},"m2"]
[null,"východní strana vnější","38,168*1,2",{"$f":"VYPOCET(C8)","v":45.801600000000001},"m2"]
[null,"severní strana vnější","(33,45+1,0+1,0+2,457+8,402+10,835+9,226+4,823+9,091+10,835+8,351+2,413+12,848+17,239)*1,1",{"$f":"VYPOCET(C9)","v":145.167},"m2"]
[null,"východní přístavba","22,026*1,3",{"$f":"VYPOCET(C10)","v":28.633800000000001},"m2"]
[null,"Převrtání stávajících injektážních otvorů včetně jejich následné výplně injektážní výplňovou hmotou",null,{"$f":"SUM(D12:D14)","v":81.5137},"m2"]
[null,"východní a severní strana vnitřní","18*1,05",{"$f":"VYPOCET(C12)","v":18.900000000000002},"m2"]
[null,"východní strana vnější","38,168*0,9",{"$f":"VYPOCET(C13)","v":34.351199999999999},"m2"]
[null,"severní strana vnější","33,25*0,85",{"$f":"VYPOCET(C14)","v":28.262499999999999},"m2"]
[null,"Nízkotlaká injektáž zdiva proti kapilárnímu vzlínání",null,{"$f":"SUM(D16)","v":26.400000000000002},"m2"]
[null,"východní a jiřní část přístavby","(12+23,2)*0,75",{"$f":"VYPOCET(C16)","v":26.400000000000002},"m2"]
[null,"SAN 01 - Minerální difúzní těsnící systém - utěsnění pod terénem",null,{"$f":"SUM(D18:D26)","v":137.64660000000001},"m2"]
[null,"jižní strana vnější","(12,2+0,8+0,8+7,0+4,8+1,0+10,9)*0,3",{"$f":"VYPOCET(C18)","v":11.25},"m2"]
[null,"západní strana vnější","66,36*0,3",{"$f":"VYPOCET(C19)","v":19.907999999999998},"m2"]
[null,"východní a severní strana vnitřní","(48,223+1+1+26,199+10,788)*0,3",{"$f":"VYPOCET(C20)","v":26.162999999999997},"m2"]
[null,"západní strana vnitřní","54,84*0,3",{"$f":"VYPOCET(C21)","v":16.452000000000002},"m2"]
[null,"jižní strana vnitřní","(1,0+6,848+4,1)*0,3",{"$f":"VYPOCET(C22)","v":3.5844},"m2"]
[null,"východní strana vnější","38,168*0,3",{"$f":"VYPOCET(C23)","v":11.4504},"m2"]
[null,"severní strana vnější","(33,45+1,0+1,0+2,457+8,402+10,835+9,226+0,8+0,8+9,091+10,835+2,413+12,848+17,239)*0,3",{"$f":"VYPOCET(C24)","v":36.118799999999993},"m2"]
[null,"východní přístavba","(12,0+22+0,8)*0,3",{"$f":"VYPOCET(C25)","v":10.44},"m2"]
[null,"otvory","(0,2+0,2+0,2+0,2+0,5+0,5+0,5+0,5+0,5+0,5+0,3+0,3+0,2+0,2)*0,3+(0,2+0,2)*0,3+(0,2+0,2)*6*0,3",{"$f":"VYPOCET(C26)","v":2.2800000000000002},"m2"]
[null,"SAN 02 - Minerální difúzně těsnící stěrka - utěsnění nad terénem pod omítkou včetně špricu",null,{"$f":"SUM(D28:D34)","v":80.446799999999996},"m2"]
[null,"jižní strana vnější","(12,2+0,8+0,8+7,0+4,8+1,0+10,9)*0,35",{"$f":"VYPOCET(C28)","v":13.125},"m2"]
[null,"západní strana vnější","66,36*0,35",{"$f":"VYPOCET(C29)","v":23.225999999999999},"m2"]
[null,"západní strana vnitřní","54,84*0,35",{"$f":"VYPOCET(C30)","v":19.193999999999999},"m2"]
[null,"jižní strana vnitřní","(1,0+6,848+4,1)*0,35",{"$f":"VYPOCET(C31)","v":4.1818},"m2"]
[null,"severní strana vnější","22,0*0,35",{"$f":"VYPOCET(C32)","v":7.6999999999999993},"m2"]
[null,"východní přístavba vnější","(12,0+22,0+0,8)*0,35",{"$f":"VYPOCET(C33)","v":12.179999999999998},"m2"]
[null,"otvory","6*0,35*(0,2+0,2)",{"$f":"VYPOCET(C34)","v":0.83999999999999986},"m2"]
[null,"SAN 03 - Minerální difúzní tesnící stěrka - vnitřní svislé utěsnění včetně špricu",null,{"$f":"SUM(D36)","v":26.661960000000001},"m2"]
[null,"východní přístavba vnitřní","(21,126+11,79)*0,81",{"$f":"VYPOCET(C36)","v":26.661960000000001},"m2"]
[null,"Přechodový a těsnící fabion",null,{"$f":"SUM(D38)","v":35.915999999999997},"bm"]
[null,"východní přístavba vnitřní","21,126+11,79+1,0+1,0+1,0",{"$f":"VYPOCET(C38)","v":35.915999999999997},"bm"]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}